{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["中文工况表","英文工况表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"中文工况表","index":0,"n_rows":37,"n_cols":5,"rows_kept":37,"merged":[[0,0,0,5],[2,0,2,5],[3,0,3,1],[3,2,3,5],[4,0,4,1],[4,2,4,3],[4,4,4,5],[5,0,5,1],[5,2,5,3],[5,4,5,5],[6,2,6,3],[6,4,6,5],[7,2,7,3],[7,4,7,5],[8,2,8,3],[8,4,8,5],[9,2,9,3],[9,4,9,5],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[14,4,14,5],[15,2,15,3],[15,4,15,5],[16,2,16,3],[16,4,16,5],[17,2,17,3],[17,4,17,5],[18,2,18,3],[18,4,18,5],[20,2,20,3],[20,4,20,5],[21,2,21,3],[21,4,21,5],[22,2,22,3],[22,4,22,5],[23,2,23,5],[24,2,24,5],[25,2,25,5],[26,2,26,5],[27,0,27,5],[28,2,28,3],[28,4,28,5],[29,2,29,3],[29,4,29,5],[30,2,30,3],[30,4,30,5],[31,2,31,3],[31,4,31,5],[32,2,32,3],[32,4,32,5],[33,2,33,3],[33,4,33,5],[34,2,34,3],[34,4,34,5],[35,2,35,5],[36,2,36,5]],"flags":["formulas_cached_only"]}
["红色栏必填 "]
[]
["碳化硅设计条件表   "]
["设备位号"]
[null,null,"夹套",null,"换热管内"]
["流体名称/组份"]
["总流量","kg/h"]
["气体流量 ","kg/h"]
["液体流量","kg/h"]
["不凝物流量 ","kg/h"]
["温度（入口/出口)","°C"]
["凝点/沸点","°C"]
["密度","kg/m3"]
["粘度","cP"]
["气体分子量","g/mol"]
["不凝物分子量","g/mol"]
["比热","cal/g/k"]
["导热系数","kcal/m/K/h"]
["潜热","kcal/kg"]
["入口压力(绝压)","Mpa"]
["流速","m/s"]
["压力降","bar"]
["污垢系数","kcal/h/m2/°C"]
["热交换量","kcal/h"]
["换热系数（干净/脏/服务侧）","kcal/h/m2/°C"]
["校正的对数平均温差","°C"]
["换热面积（需要的/提供的）","m2"]
["设备选型数据"]
["设计温度","°C"]
["设计压力","barg"]
["测试压力","barg"]
["程数"]
["入口管道直径","mm"]
["出口管道直径","mm"]
["材料"]
["重量（空/满水）","kg"]
["安装方式"]

{"sheet":"英文工况表","index":1,"n_rows":37,"n_cols":5,"rows_kept":37,"merged":[[0,0,0,5],[2,0,2,5],[3,0,3,1],[3,2,3,5],[4,0,4,1],[4,2,4,3],[4,4,4,5],[5,0,5,1],[5,2,5,3],[5,4,5,5],[6,2,6,3],[6,4,6,5],[7,2,7,3],[7,4,7,5],[8,2,8,3],[8,4,8,5],[9,2,9,3],[9,4,9,5],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[14,4,14,5],[15,2,15,3],[15,4,15,5],[16,2,16,3],[16,4,16,5],[17,2,17,3],[17,4,17,5],[18,2,18,3],[18,4,18,5],[20,2,20,3],[20,4,20,5],[21,2,21,3],[21,4,21,5],[22,2,22,3],[22,4,22,5],[23,2,23,5],[24,2,24,5],[25,2,25,5],[26,2,26,5],[27,0,27,5],[28,2,28,3],[28,4,28,5],[29,2,29,3],[29,4,29,5],[30,2,30,3],[30,4,30,5],[31,2,31,3],[31,4,31,5],[32,2,32,3],[32,4,32,5],[33,2,33,3],[33,4,33,5],[34,2,34,3],[34,4,34,5],[35,2,35,5],[36,2,36,5]],"flags":["formulas_cached_only"]}
["Red column must be filled"]
[]
["   Design requests of SIC"]
["Device number"]
[null,null,"Jacket",null,"in side of heat exchanger"]
["Fluid name / component*FluiFluid name / componentd name / component"]
["Total flow*","kg/h"]
["Gas flow","kg/h"]
["Liquid flow","kg/h"]
["Non condensable material flow","kg/h"]
["Tempreture ( In / Out)","°C"]
["Freezing point / Boiling point","°C"]
["Density","kg/m3"]
["Viscosity","cP"]
["Gas molecular weigh","g/mol"]
["Molecular weight of non condensates","g/mol"]
["Specific heat","cal/g/k"]
["Thermal conductivity","kcal/m/K/h"]
["latent heat","kcal/kg"]
["Inlet pressure (absolute pressure)","Mpa"]
["Current Speed","m/s"]
["Pressure drop","bar"]
["Fouling coefficient","kcal/h/m2/°C"]
["Heat exchange capacity","kcal/h"]
["Heat transfer coefficient (clean / dirty / service side)","kcal/h/m2/°C"]
["Corrected logarithmic mean temperature difference","°C"]
["Heat exchange area (required / provided)","m2"]
["Equipment selection data"]
["Design temperature","°C"]
["Design pressure","barg"]
["Test pressure","barg"]
["Process number"]
["Inlet pipe diameter","mm"]
["Outlet pipe diameter","mm"]
["Material"]
["Weight (empty / full water)","kg"]
["Installation method"]